      Icons web 25px9

|  |  |
| --- | --- |
| **Agency Contact:**  Miranda Warren  Wall Street Communications  Tel: +1 (631) 681-7475  Email: miranda@wallstcom.com | **Riedel Communications Contact:**  Serkan Güner  Marketing and Communications  Tel: + 49 174 33 92 448  Email: press@riedel.net |

**Link to Word Doc:** [www.wallstcom.com/Riedel/240326-Riedel-JP\_Morgan-TSL.docx](https://www.wallstcom.com/Riedel/240326-Riedel-JP_Morgan-TSL.docx)

**Photo Links:** www.wallstcom.com/Riedel/

**Photo Caption:** Riedel FusioN Edge Devices

**Photo Link:** www.wallstcom.com/Rieldel/

**Photo Caption:** Riedel and TSL Deployment in Leading Financial Services Firm

**Riedel与TSL联手为知名金融公司提供高性价比、高质量的视频路由和控制系统**

WUPPERTAL，德国 – 2024年3月26日 – Riedel Communications今日宣布，通过与TSL的战略合作成功部署了一套灵活、高性价比的视频分发和控制系统，并将其部署于某知名金融服务公司内。系统集成商 Diversified 提供了此套解决方案，其中Riedel的 MediorNet IP 视频分发和转换设备与TSL屡获殊荣的 X-Connect SMPTE ST 2110 路由控制解决方案及虚拟面板界面相结合，在无需大型视频矩阵的情况下实现了专业级的分布式 IP 路由和控制。

此套系分别布署在用户的两个主要办公场所，超过50台Riedel MediorNet FusioN 边缘设备在TSL X-Connect 的配置下，形成了一个灵活的小规模解决方案。FusioN在此不仅承担 3G/UHD SDI/IP 网关功能，还针对财富管理会议、客户会议和实时网络研讨会等需要高质量视频和简单易用的使用场景进行了针对性定制。

此外，FusioN还将承担 PTZ 摄像机控制的以太网隧道载体，满足摄像机操作员的远程无缝控制需求。同时，FusioN为客户带来可选的 BB同步信号输出和帧同步功能，便于灵活地通过 BB 输出同步远端设备，或在IP封装过程中利用帧同步将异步信号源锁定至系统 PTP同步域内。此外，核心 IP 媒体架构由两对 MediorNet VirtU-48 组成，以此建立冗余网络架构，通过 SMPTE ST 2022-7 无缝保护切换确保信号完全冗余，打造高容错高可用网络。而依托于TSL X-Connect ST 2110 路由解决方案，可以轻松连接和控制 IP 边缘设备和传统广电设备，从而弥合 SDI 和 IP 工作流程之间的相互集成互联的诸多障碍。

“在不断演变的 IP 领域，各种规模的内容制作商和播出商都开始选择使用开放且经济实惠的解决方案，利用 IP 和商用产品 (COTS) 的优势，从而避免昂贵的大规模基础设施改造，” TSL公司总裁兼控制部门主管 Ian Godfrey 表示：“通过将 X-Connect 与Riedel创新的 MediorNet IP 视频系统的集成，我们创造了一个简单易用的解决方案，可在客户整个公司内进行高质量的视频分发。”

这家金融服务公司是Riedel近期的新客户，他们利用这项联合解决方案轻松地在公司内传输大量视频信号。尽管该项目最初设计时没有考虑控制系统，但最终部署的系统为整个公司带来了更具灵活性的架构以及高品质控制和 tally 功能，可以满足公司多功能厅、现场活动中心以及通过 Zoom 等第三方平台进行虚拟观众互动等方面的需求。

“Riedel和TSL的合作在为客户提供高性价比且专业的视频路由和控制解决方案中，发挥了重要作用，”Riedel东区区域销售总监 Dave Caulwell 表示，“客户非常喜欢 FusioN 边缘设备的小巧外观以及可适用于各种终端设备的多样化I/O 选项。我们与TSL创新的控制系统相结合，最终产生的系统能够充分填补行业空白，为企业空间量身定制了高质量的视频解决方案。”

Further information about Riedel and the company’s products is available at [www.riedel.net](http://www.riedel.net/).

# # #

**About TSL**

For over 30 years we have worked directly with the world's leading broadcasters and content creators to design, manufacture and market a range of broadcast workflow solutions that serve to simplify operations within the television broadcast, cable, satellite, IPTV and IT industries. Specializing in audio monitoring, broadcast control systems and power management tools, we ensure that our solutions satisfy and exceed the commercial, technical and operational requirements that exist in IT-based and traditional workflows to help our customers lower costs, generate revenue and streamline operations.

**About Riedel Communications**

Riedel Communications is a leading provider of live production tools in the worlds of media, sports, and entertainment. The company's hard- and software solutions span from distributed video and audio networks over intercom and replay solutions to WAN and MPLS applications. Thanks to Riedel's holistic approach, its three business units — Product Division, Managed Technology Division and Networks Division — can leverage powerful synergies to provide flexible infrastructures, tools, and services for both fixed and temporary installations around the globe, enabling Riedel customers to run even the most complex projects on-site, remotely, or in the cloud. Riedel is headquartered in Wuppertal, Germany, and employs over 1,000 people in 30 locations throughout Europe, Australia, Asia, and the Americas.  
   
*All trademarks appearing herein are the property of their respective owners.*