      Icons web 25px9

|  |  |
| --- | --- |
| **Agency Contact:**  Sunny Branson  Wall Street Communications  Tel: +1 801 326 9946  Email: sunny@wallstcom.com | **Riedel Communications Contact:**  Serkan Güner  Marketing and Communications  Tel: + 49 174 33 92 448  Email: press@riedel.net |

**Link to Word Doc:** [www.wallstcom.com/Riedel/240413-Riedel-RiCapture.docx](https://www.wallstcom.com/Riedel/240413-Riedel-RiCapture.docx)

**Photo Links:**

[www.wallstcom.com/Riedel/RiCapturePR.jpg](https://www.wallstcom.com/Riedel/RiCapturePR.jpg)

[www.wallstcom.com/Riedel/RiCaptureUI-Servers.jpg](https://www.wallstcom.com/Riedel/RiCaptureUI-Servers.jpg)

**Photo Caption:** New additions to Riedel RiCapture lineup bring increased channel density, 8- and 10-bit support, greater internal SSD storage, and more.

**Riedel Expands RiCapture Ingest Solutions Portfolio With Release of i8, i44, and i84**

**WUPPERTAL, Germany** — **April 13, 2024** — At the 2024 NAB Show, Riedel Communications announced a significant expansion of the company’s RiCapture ingest solutions line with the addition of RiCapture i8, i44, and i84. Complementing the RiCapture i4, these new additions bring increased channel density and/or UHD resolution, 8- and 10-bit support, expanded internal SSD storage, and a series of advanced functionalities to the RiCapture platform.

With the brand-new SSE interface for scheduling, streaming, and exporting, the RiCapture product line now offers a powerful and compact solution for multichannel HD/UHD ingest recording and integration to postproduction. The SSE control application allows for flexible configuration, letting users select between high-resolution DNxHD/R, H.264, or a combination of the two and includes audio-mapping and down-mix audio-listening capabilities. RiCapture offers maximum versatility to capture the recorded media locally, on removable storage, on network-attached storage, or to live-streaming destinations. It can be expanded to a network of multiple servers for higher-density recording and unlimited destinations with control from a single SSE interface.

The i4 and i8 provide four or eight HD HDR input channels, while the i44 and i84 boast four UHD channels with HDR capability. On the audio side, all RiCapture products are capable of 16 channels of embedded audio per channel, as well as 64 Dante or AES67 channels.

In all configurations, RiCapture offers high-quality recording in DNxHD or DNxHR along with H.264 4:2:0 and 4:2:2 encoding to the local storage. The local recording storage offers continuous loop recording for the captured content, with options to stream manually, stream with a scheduler, or clip and export files as needed from the available local storage to numerous streaming destinations.

There are three software add-ons available in the RiCapture product line: the VDR panel, a web-based UI with expanded multichannel control for clip playback, program delays, monitor wall playback and other scenarios; the RiView application, which is a multiviewer UI that includes audio down-mix monitoring for synchronized review of record feeds for review, clipping, and export to multiple destinations; and the XDCAM add-on, which provides the tapeless XDCAM format for HD video acquisition and storage.

“As a complete suite for multichannel ingest recording capture and transfer to postproduction, RiCapture caters to a wide range of markets — from sports, concerts, and theaters to motion picture applications,” said Bernard Stas, Product Manager, Live Video Production, Riedel Communications. “Accommodating UHD resolutions and a variety of formats, such as 23.98 fps and 29.97 fps, the newly expanded RiCapture family sets the bar for high-quality ingest solutions at an exceptionally competitive price.”

Further information about Riedel and the company’s products is available at [www.riedel.net](http://www.riedel.net/).

# # #

**About Riedel Communications**

Riedel Communications is a leading provider of live production tools in the worlds of media, sports, and entertainment. The company's hard- and software solutions span from distributed video and audio networks over intercom and replay solutions to WAN and MPLS applications. Thanks to Riedel's holistic approach, its three business units — Product Division, Managed Technology Division and Networks Division — can leverage powerful synergies to provide flexible infrastructures, tools, and services for both fixed and temporary installations around the globe, enabling Riedel customers to run even the most complex projects on-site, remotely, or in the cloud. Riedel is headquartered in Wuppertal, Germany, and employs over 1,000 people in 30 locations throughout Europe, Australia, Asia, and the Americas.  
   
*All trademarks appearing herein are the property of their respective owners.*